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Supply Grilles & Registers



DA821
SINGLE DEFLECTION SUPPLY REGISTER - VERTICAL BLADE - MULTI-SHUTTER

MODEL DESCRIPTION: Single deflection supply register with vertical blades and multi-shutter damper.
TYPE: Supply register.
BLADE ARRANGEMENT: One set of individually adjustable, semi-airfoil vertical blades spaced on 2/3 in. centers. 
DAMPER: Multi-shutter damper with easily accessible handle.
FRAME: Standard architectural aluminum frame.
FINISHES: W - White; S - Silver; M – Mill
PERFORMANCE BASIS: ANSI/ASHRAE Standard 70-2023
SUGGESTED SPECIFICATION
Furnish and install Dayus Model DA821 Single Deflection Supply Registers of the type, finish, listed size/opening size, and mounting method shown on the plans and air distribution schedules. The registers shall have one set of individually adjustable, semi-airfoil vertical blades spaced on 2/3 in. centers. The frame shall be architectural aluminum with roll-formed aluminum blades, pressure-fitted for rattle-free performance, and supplied with a sealing gasket to help prevent streaking on walls or ceilings. The register shall include a multi-shutter damper with easily accessible handle for volume control. Units shall be furnished in Dayus W White, S Silver, or M Mill finish as scheduled.
(Optional) No screw-hole fastening shall be provided where scheduled. Where an opposed blade damper is required, provide Dayus Model DAVD.
The manufacturer shall provide published performance data for the grille or register, which shall be tested in accordance with ANSI/ASHRAE Standard 70-2023.
STANDARD FEATURES
· Individually adjustable, semi-airfoil vertical blades on 2/3 in. spacing
· Architectural aluminum construction with extruded frame and roll-formed blades
· Pressure-fitted blades for rattle-free performance
· Sealing gasket to help prevent streaking on walls or ceilings
· Available on 2 in. standard dimensions; custom sizes manufactured up to 1/16 in. increments.
RELATED OPTIONS / MODEL VARIANTS
· DA821-TB - No screw holes
· DAVD - Opposed blade damper
· DAHM - Horizontal blade version
Note: Use bracketed finish, size, mounting, and option selections from the project plans and air distribution schedule.
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