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DABL-FG4
4" BAR LINEAR FILTER GRILLE

TYPE: 4 in. bar linear face filter grille.
BLADE ARRANGEMENT: Fixed bar linear blades parallel to the long dimension unless otherwise scheduled, with blade option selected from -00, -01, -15, -30, -82, or -84.
DAMPER / FILTER / SCREEN: Integral filter frame for 4 in. filter; mounting selected as scheduled.
FRAME: Fully extruded architectural aluminum frame with bar linear face and filter frame 
FINISHES: W White; S Silver; M Mill.
PERFORMANCE BASIS: ANSI/ASHRAE Standard 70-2023
SUGGESTED SPECIFICATION
Furnish and install Dayus Model DABL-FG4 4" Bar Linear Filter Grille of the type, finish, scheduled listed size/opening size, outside size, or inside size as applicable, and mounting method shown on the plans and air distribution schedules.
The bar linear face filter grille shall be constructed with fully extruded architectural aluminum frame with bar linear face and filter frame and fixed bar linear blades parallel to the long dimension unless otherwise scheduled, with blade option selected from -00, -01, -15, -30, -82, or -84.
The unit shall include an integral filter frame for 4 in. filter; mounting selected as scheduled.
Units shall be furnished in Dayus [W White; S Silver; M Mill] finish as scheduled.
Provide scheduled options and related model variants as indicated.
The manufacturer shall provide published performance data for the bar linear filter grille, which shall be tested in accordance with ANSI/ASHRAE Standard 70-2023.
STANDARD FEATURES
· Bar linear face with selectable blade profile
· Accommodates a standard 4 in. filter
· Top and bottom mounting options: spring pins, Wire Hinge, Nylon Thumb Screw, Nylon Screen Tabs, or security screws as scheduled
· Recommended top mounting: spring pins or Wire Hinge only
· Available on 2 in. standard dimensions; custom sizes to 1/16 in. increments
RELATED OPTIONS / MODEL VARIANTS
· Spring pin, Wire Hinge, Nylon Thumb Screw, Nylon Screen Tab, or Security Screw bottom mounting as scheduled; use Spring Pin or Wire Hinge for top mounting
· T-bar ceiling frame variant available where scheduled
· 1 in or 2 in. filter depth variants
Note: Confirm listed size/opening size, outside size, or inside size as applicable; finish; mounting method; damper/filter/screen requirements; and current Dayus model availability before issuing project specifications.
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