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DABLC
BAR LINEAR CORE

TYPE: Bar linear core.
BLADE ARRANGEMENT: Fixed bars parallel to the long dimension unless otherwise scheduled; blade option selected from -00, -01, -15, -30, -82, or -84.
DAMPER / FILTER / SCREEN: None. 
FRAME: Core-only construction; frame, mounting hardware, and damper not included unless scheduled separately.
FINISHES: W White; S Silver; M Mill; B- Brown; FB – Flat Black; P – Prime Coat; Special Order.
PERFORMANCE BASIS: ANSI/ASHRAE Standard 70-2023
SUGGESTED SPECIFICATION
Furnish and install Dayus Model DABLC Bar Linear Core of the type, finish, scheduled listed size/opening size, outside size, or inside size as applicable, and mounting method shown on the plans and air distribution schedules.
The bar linear core shall be constructed with core-only construction; frame, mounting hardware, and damper not included unless scheduled separately; fixed bars shall be parallel to the long dimension unless otherwise scheduled; blade option selected from -00, -01, -15, -30, -82, or -84. Provide -F Reinforced Floor option where scheduled for floor applications.
Units shall be furnished in Dayus [White; Silver; Mill; Brown; Flat Black; Prime Coat; Custom] finish as scheduled.
Provide scheduled options and related model variants as indicated.
The manufacturer shall provide published performance data for the bar linear core, which shall be tested in accordance with ANSI/ASHRAE Standard 70-2023.
STANDARD FEATURES
· Core-only bar linear section for installation in a separate frame or prepared opening
· Fixed bars parallel to long dimension unless otherwise scheduled
· Six blade profile options: -00, -01, -15, -30, -82, -84
· Fully extruded architectural aluminum construction
· -F Reinforced Floor option available where scheduled
· 1/2 in. standard dimensions; custom sizes to 1/16 in. increments
RELATED OPTIONS / MODEL VARIANTS
· -F Reinforced Floor option available where scheduled
· DABL - Standard frame grille
· DABLD - Standard frame register with opposed blade damper
· DABLCF - Floor-rated bar linear floor core where scheduled
Note: Confirm listed size/opening size, outside size, or inside size as applicable; finish; mounting method; damper/filter/screen requirements; and current Dayus model availability before issuing project specifications. 
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