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DABLDJ
BAR LINEAR REGISTER WITH MUD-IN FLANGE

TYPE: Bar linear register.
BLADE ARRANGEMENT: Fixed bars parallel to the long dimension unless otherwise scheduled; blade option selected from -00, -01, -15, -30, -82, or -84.
DAMPER / FILTER / SCREEN: Opposed blade damper with concealed operator design.
FRAME: Fully extruded architectural aluminum, recessed mud-in flange frame.
FINISHES: W White; S Silver; M Mill; B- Brown; FB – Flat Black; P – Prime Coat; Special Order.
PERFORMANCE BASIS: ANSI/ASHRAE Standard 70-2023
SUGGESTED SPECIFICATION
Furnish and install Dayus Model DABLDJ Bar Linear Register with mud-in flange of the type, finish, scheduled listed size/opening size, outside size, or inside size as applicable, and mounting method shown on the plans and air distribution schedules.
The bar linear register shall be constructed with fully extruded architectural aluminum recessed mud-in flange frame and fixed bars parallel to the long dimension unless otherwise scheduled; blade option selected from -00, -01, -15, -30, -82, or -84.
The unit shall include an opposed blade damper with concealed operator design.
Units shall be furnished in Dayus [White; Silver; Mill; Brown; Flat Black; Prime Coat; Custom] finish as scheduled.
Provide scheduled options and related model variants as indicated.
The manufacturer shall provide published performance data for the bar linear register, which shall be tested in accordance with ANSI/ASHRAE Standard 70-2023.
STANDARD FEATURES
· Concealed mud-in flange for tape-and-plaster installation
· Fixed bar blades, direction as scheduled
· Six blade profile options: -00, -01, -15, -30, -82, -84
· Fully extruded architectural aluminum construction
· 1/2 in. standard dimensions; custom sizes to 1/16 in. increments
· Not designed for floor use unless a floor-rated model is specifically scheduled
RELATED OPTIONS / MODEL VARIANTS
· Opposed blade damper with concealed operator
· DABLJ - No-damper mud-in flange grille
· DABLDRJ - Removable-core mud-in flange register
Note: Confirm listed size/opening size, outside size, or inside size as applicable; finish; mounting method; damper/filter/screen requirements; and current Dayus model availability before issuing project specifications. 
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