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DABLS
SHALLOW BAR LINEAR GRILLE

TYPE: Shallow bar linear grille.
BLADE ARRANGEMENT: Fixed bars parallel to the long dimension; 0.094” blades on ½” centers.
DAMPER / FILTER / SCREEN: None. 
FRAME: Fully extruded architectural aluminum, standard extruded aluminum frame, slim 1/2 in. deep profile.
FINISHES: W White; S Silver; M Mill; B- Brown; FB – Flat Black; P – Prime Coat; Special Order.
PERFORMANCE BASIS: None. 
SUGGESTED SPECIFICATION
Furnish and install Dayus Model DABLS Shallow Bar Linear Grille of the type, finish, scheduled listed size/opening size, outside size, or inside size as applicable, and mounting method shown on the plans and air distribution schedules.
The shallow bar linear grille shall be constructed with fully extruded architectural aluminum standard frame with slim 1/2 in. deep profile and fixed bars parallel to the long dimension unless otherwise scheduled; 0.094” blades on ½” centers.
Units shall be furnished in Dayus [White; Silver; Mill; Brown; Flat Black; Prime Coat; Custom] finish as scheduled.
Provide scheduled options and related model variants as indicated.
STANDARD FEATURES
· Slim 1/2 in. deep design
· Fixed bars parallel to long dimension
· 0.094” blades on ½” centers.
· Selectable 2, 3, 4, or 6 in. height
· Fully extruded architectural aluminum construction
· Not designed for floor use
· 1/2 in. standard dimensions; custom sizes to 1/16 in. increments
Note: Confirm listed size/opening size, outside size, or inside size as applicable; finish; mounting method; damper/filter/screen requirements; and current Dayus model availability before issuing project specifications.
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