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Supply Grilles & Registers



DAHD
SINGLE DEFLECTION SUPPLY REGISTER - HORIZONTAL BLADE - OBD

MODEL DESCRIPTION: Single deflection aluminum register with horizontal blades and opposed blade damper. 
TYPE: Supply register. 
BLADE ARRANGEMENT: One set of individually adjustable, semi-airfoil horizontal blades spaced on 2/3 in. centers.
DAMPER: Opposed blade damper with concealed operator design.
FRAME: Standard architectural aluminum frame.
FINISHES: W - White; S - Silver; M – Mill
PERFORMANCE BASIS: ANSI/ASHRAE Standard 70-2023
SUGGESTED SPECIFICATION
Furnish and install Dayus Model DAHD Single Deflection Supply Registers of the type, finish, listed size/opening size, and mounting method shown on the plans and air distribution schedules. The registers shall have one set of individually adjustable, semi-airfoil horizontal blades spaced on 2/3 in. centers. The frame shall be architectural aluminum with roll-formed aluminum blades, pressure-fitted for rattle-free performance, and supplied with a sealing gasket to help prevent streaking on walls or ceilings. The register shall include an opposed blade damper with concealed operator design for volume control. Units shall be furnished in Dayus W White, S Silver, or M Mill finish as scheduled.
(Optional) No screw-hole fastening and all-aluminum construction shall be provided where scheduled. Where a damper is not required, provide Dayus Model DAH.
The manufacturer shall provide published performance data for the grille or register, which shall be tested in accordance with ANSI/ASHRAE Standard 70-2023.
STANDARD FEATURES
· Individually adjustable, semi-airfoil horizontal blades on 2/3 in. spacing
· Architectural aluminum construction with extruded frame and roll-formed blades
· Pressure-fitted blades for rattle-free performance
· Sealing gasket to help prevent streaking on walls or ceilings
· Available on 2 in. standard dimensions; custom sizes manufactured up to 1/16 in. increments.
RELATED OPTIONS / MODEL VARIANTS
· DAHD-TB - No screw holes
· DAHD-AA - All aluminum construction
· DAH - No damper
· DAVD - Vertical blade version
Note: Use bracketed finish, size, mounting, and option selections from the project plans and air distribution schedule.
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