How to Specify
 
Specify
 SPECIFY

Supply Grilles & Registers



DAHV
DOUBLE DEFLECTION SUPPLY GRILLE - HORIZONTAL FRONT

MODEL DESCRIPTION: Double deflection aluminum grille with horizontal front blades and vertical rear blades.
TYPE: Supply grille.
BLADE ARRANGEMENT: Two sets of individually adjustable, semi-airfoil blades spaced on 2/3 in. centers; horizontal front blades and vertical rear blades.
DAMPER: None.
FRAME: Standard architectural aluminum frame.
FINISHES: W - White; S - Silver; M – Mill
PERFORMANCE BASIS: ANSI/ASHRAE Standard 70-2023
SUGGESTED SPECIFICATION
Furnish and install Dayus Model DAHV Double Deflection Supply Grilles of the type, finish, listed size/opening size, and mounting method shown on the plans and air distribution schedules. The grilles shall have two sets of individually adjustable, semi-airfoil blades spaced on 2/3 in. centers, with horizontal front blades and vertical rear blades for two-plane air-direction control. The frame shall be architectural aluminum with roll-formed aluminum blades, pressure-fitted for rattle-free performance, and supplied with a sealing gasket to help prevent streaking on walls or ceilings. Units shall be furnished in Dayus W White, S Silver, or M Mill finish as scheduled.
(Optional) No screw-hole fastening and all-aluminum construction shall be provided where scheduled. Where a damper is required, provide Dayus Model DAHVD.
The manufacturer shall provide published performance data for the grille or register, which shall be tested in accordance with ANSI/ASHRAE Standard 70-2023.
STANDARD FEATURES
· Two sets of individually adjustable, semi-airfoil blades with horizontal front blades and vertical rear blades on 2/3 in. spacing
· Architectural aluminum construction with extruded frame and roll-formed blades
· Pressure-fitted blades for rattle-free performance
· Sealing gasket to help prevent streaking on walls or ceilings
· Available on 2 in. standard dimensions; custom sizes manufactured up to 1/16 in. increments.
RELATED OPTIONS / MODEL VARIANTS
· DAHVD - Opposed blade damper
· DAHV-TB - No screw holes
· DAHV-AA - All aluminum construction
· DAVH - Vertical front version
Note: Use bracketed finish, size, mounting, and option selections from the project plans and air distribution schedule.
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