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DAL2-WF
2" STATIONARY LOUVER WITH WIDE FLANGE

TYPE: 2 in. stationary louver with wide flange frame.
BLADE ARRANGEMENT: Fixed non-drainable blades on 2 in. spacing with J-blade design; nominal 43% free area based on 48 in. x 48 in. louver.
DAMPER / FILTER / SCREEN: Bird screen standard; insect screen optional where scheduled.
FRAME: Heavy-duty extruded aluminum wide flange frame.
FINISHES: White; Silver; Mill; Brown; Flat Black; Prime Coat; Custom
PERFORMANCE BASIS: AMCA Standard 500-L
SUGGESTED SPECIFICATION
Furnish and install Dayus Model DAL2-WF 2" Stationary Louver with Wide Flange of the type, finish, scheduled listed size/opening size, outside size, or inside size as applicable, and mounting method shown on the plans and air distribution schedules.
The 2 in. stationary louver with wide flange frame shall be constructed with heavy-duty extruded aluminum wide flange frame and fixed non-drainable blades on 2 in. spacing with J-blade design; nominal 43% free area based on 48 in. x 48 in. louver.
The louver shall be supplied with bird screen standard; insect screen shall be optional where scheduled.
Units shall be furnished in Dayus [White; Silver; Mill; Brown; Flat Black; Prime Coat; Custom] finish as scheduled.
Provide scheduled options and related model variants as indicated.
The manufacturer shall provide published performance data for the louver, which shall be tested in accordance with AMCA Standard 500-L.
STANDARD FEATURES
· 2 in. fixed-blade stationary louver
· J-blade design to minimize water ingress
· Nominal 43% free area based on 48 in. x 48 in. louver
· Mullions for sizes over 36 in. length
· Bird screen standard; insect screen optional
· AAMA 2605 high-performance exterior finish available
RELATED OPTIONS / MODEL VARIANTS
· Insect screen where scheduled
· Alternate frame style where available
· Extended louver sill where applicable
Note: Confirm listed size/opening size, outside size, or inside size as applicable; finish; mounting method; damper/filter/screen requirements; and current Dayus model availability before issuing project specifications. 
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