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DAL4-CF
4" STATIONARY LOUVER WITH CHANNEL FRAME

TYPE: 4 in. non-drainable stationary louver with channel frame.
BLADE ARRANGEMENT: J-blade fixed louver design; nominal 48% free area.
DAMPER / FILTER / SCREEN: Bird screen standard; insect screen optional where scheduled.
FRAME: Heavy-duty extruded aluminum channel frame.
FINISHES: White; Silver; Mill; Brown; Flat Black; Prime Coat; Custom
PERFORMANCE BASIS: AMCA Standard 500-L
SUGGESTED SPECIFICATION
Furnish and install Dayus Model DAL4-CF 4" Stationary Louver with Channel Frame of the type, finish, scheduled listed size/opening size, outside size, or inside size as applicable, and mounting method shown on the plans and air distribution schedules.
The 4 in. non-drainable stationary louver with channel frame shall be constructed with heavy-duty extruded aluminum channel frame and J-blade fixed louver design; nominal 48% free area.
The louver shall be supplied with bird screen standard; insect screen shall be optional where scheduled.
Units shall be furnished in Dayus [White; Silver; Mill; Brown; Flat Black; Prime Coat; Custom] finish as scheduled.
Provide scheduled options and related model variants as indicated.
The manufacturer shall provide published performance data for the louver, which shall be tested in accordance with AMCA Standard 500-L.
STANDARD FEATURES
· 4 in. non-drainable fixed-blade louver
· J-blade design to minimize water ingress
· Nominal 48% free area
· Concealed mullions for sizes over 48 in. length
· Bird screen standard; insect screen optional
· AAMA 2604 powder coat; AAMA 2605 architectural finish available
RELATED OPTIONS / MODEL VARIANTS
· Insect screen where scheduled
· Alternate frame style where available
· Extended louver sill where applicable
Note: Confirm listed size/opening size, outside size, or inside size as applicable; finish; mounting method; damper/filter/screen requirements; and current Dayus model availability before issuing project specifications. 
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