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DANV
TRANSFER / DOOR GRILLE

TYPE: Transfer / door grille.  
BLADE ARRANGEMENT: Inverted V-shaped horizontal blades on 2/3 in. spacing to minimize sightlines while maintaining free area. 
DAMPER / FILTER / SCREEN: None.
FRAME: Architectural aluminum frame with pressure-fitted roll-formed blades
FINISHES: W - White; S - Silver; M - Mill
PERFORMANCE BASIS: ANSI/ASHRAE Standard 70-2023
SUGGESTED SPECIFICATION
Furnish and install Dayus Model DANV Transfer/Door Grille of the type, finish, scheduled listed size/opening size, outside size, or inside size as applicable, and mounting method shown on the plans and air distribution schedules.
The Transfer / door grille shall be constructed with architectural aluminum frame with pressure-fitted roll-formed blades and inverted V-shaped horizontal blades on 2/3 in. spacing to minimize sightlines while maintaining free area.
Units shall be furnished in Dayus [W White; S Silver; M Mill] finish as scheduled.
Provide scheduled options and related model variants as indicated.
The manufacturer shall provide published performance data for the transfer grille, which shall be tested in accordance with ANSI/ASHRAE Standard 70-2023.
STANDARD FEATURES
· Inverted V-blade design for reduced sightlines
· Horizontal blades on 2/3 in. spacing
· Architectural aluminum construction
· Available with auxiliary frame or No mounting option
RELATED OPTIONS / MODEL VARIANTS
· DANV-A with auxiliary frame
· DANV-B grille only
Note: Confirm listed size/opening size, outside size, or inside size as applicable; finish; mounting method; damper/filter/screen requirements; and current Dayus model availability before issuing project specifications.
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