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DAPH
HEAVY DUTY BAR LINEAR GRILLE

TYPE: Heavy duty bar linear grille.
BLADE ARRANGEMENT: Fixed bars parallel to the long dimension unless otherwise scheduled; blade option selected from -00, -01, -15, -30, -82, or -84.
DAMPER / FILTER / SCREEN: None. 
FRAME: Fully extruded architectural aluminum frame; reinforced heavy-duty core with additional supports every 2 in.
FINISHES: W White; S Silver; M Mill; B- Brown; FB – Flat Black; P – Prime Coat; Special Order.
PERFORMANCE BASIS: ANSI/ASHRAE Standard 70-2023
SUGGESTED SPECIFICATION
Furnish and install Dayus Model DAPH Heavy Duty Bar Linear Grille of the type, finish, scheduled listed size/opening size, outside size, or inside size as applicable, and mounting method shown on the plans and air distribution schedules.
The heavy-duty bar linear grille shall be constructed with fully extruded architectural aluminum frame; reinforced heavy-duty core with additional supports every 2 in. and fixed bars parallel to the long dimension unless otherwise scheduled; blade option selected from -00, -01, -15, -30, -82, or -84.
Units shall be furnished in Dayus [White; Silver; Mill; Brown; Flat Black; Prime Coat; Custom] finish as scheduled.
Provide scheduled options and related model variants as indicated.
The manufacturer shall provide published performance data for the bar linear grille, which shall be tested in accordance with ANSI/ASHRAE Standard 70-2023.
STANDARD FEATURES
· Fixed bars parallel to long dimension unless otherwise scheduled
· Reinforced heavy-duty core with additional supports every 2 in.
· Designed for floor or reinforced sidewall, sill, and ceiling applications
· Fully extruded architectural aluminum construction
· 1/2 in. standard dimensions; custom sizes to 1/16 in. increments
RELATED OPTIONS / MODEL VARIANTS
· DAPHD - Opposed blade damper/register
· DAPHN - No-flange heavy-duty grille
· DAPHC - Heavy-duty core only
· DAPH-TB - No mounting / No screw-hole option where scheduled
Note: Confirm listed size/opening size, outside size, or inside size as applicable; finish; mounting method; damper/filter/screen requirements; and current Dayus model availability before issuing project specifications.
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