How to Specify
 
Specify
 SPECIFY

Bar Linear



DAPHC 
HEAVY DUTY BAR LINEAR CORE 

TYPE: Heavy duty bar linear core. 
BLADE ARRANGEMENT: Fixed bars parallel to the long dimension unless otherwise scheduled; blade option selected from -00, -01, -15, -30, -82, or -84.
DAMPER / FILTER / SCREEN: None. 
FRAME: Fully extruded architectural aluminum, core-only construction, reinforced heavy-duty core with additional supports.
FINISHES: W White; S-Silver; M-Mill; B-Brown; FB-Flat Black; P-Prime Coat; Special Order.
PERFORMANCE BASIS: ANSI/ASHRAE Standard 70-2023
SUGGESTED SPECIFICATION
Furnish and install Dayus Model DAPHC Heavy Duty Bar Linear Core of the type, finish, scheduled listed size/opening size, outside size, or inside size as applicable, and mounting method shown on the plans and air distribution schedules.
The heavy-duty bar linear core shall be constructed with fully extruded architectural aluminum core-only construction, reinforced heavy-duty core with additional supports and fixed bars parallel to the long dimension unless otherwise scheduled; blade option selected from -00, -01, -15, -30, -82, or -84.
Units shall be furnished in Dayus [White; Silver; Mill; Brown; Flat Black; Prime Coat; Custom] finish as scheduled.
Provide scheduled options and related model variants as indicated.
The manufacturer shall provide published performance data for the bar linear core, which shall be tested in accordance with ANSI/ASHRAE Standard 70-2023.
STANDARD FEATURES
· Heavy-duty core-only bar linear section
· Fixed bars parallel to long dimension unless otherwise scheduled
· Reinforced heavy-duty core with additional supports
· Fully extruded architectural aluminum construction
· 1/2 in. standard dimensions; custom sizes to 1/16 in. increments
RELATED OPTIONS / MODEL VARIANTS
· DAPH - Heavy-duty grille with frame
· DAPHD - Heavy-duty register with opposed blade damper
Note: Confirm listed size/opening size, outside size, or inside size as applicable; finish; mounting method; damper/filter/screen requirements; and current Dayus model availability before issuing project specifications. 
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