How to Specify
 
Specify
 SPECIFY

Bar Linear



DABLS
SHALLOW BAR LINEAR GRILLE

TYPE: Shallow bar linear grille.
BLADE ARRANGEMENT: Fixed bars parallel to the long dimension unless otherwise scheduled; blade option selected from -00, -01, -15, -30, -82, or -84.
DAMPER / FILTER / SCREEN: Opposed blade damper with concealed operator design.
FRAME: Fully extruded architectural aluminum frame; reinforced heavy-duty core with additional supports every 2 in.
FINISHES: W White; S Silver; M Mill; B- Brown; FB – Flat Black; P – Prime Coat; Special Order.
PERFORMANCE BASIS: ANSI/ASHRAE Standard 70-2023
SUGGESTED SPECIFICATION
Furnish and install Dayus Model DAPHD Heavy Duty Bar Linear Register of the type, finish, scheduled listed size/opening size, outside size, or inside size as applicable, and mounting method shown on the plans and air distribution schedules.
The heavy-duty bar linear register shall be constructed with fully extruded architectural aluminum frame; reinforced heavy-duty core with additional supports every 2 in. and fixed bars parallel to the long dimension unless otherwise scheduled; blade option selected from -00, -01, -15, -30, -82, or -84.
The unit shall include an opposed blade damper with concealed operator design.
Units shall be furnished in Dayus [White; Silver; Mill; Brown; Flat Black; Prime Coat; Custom] finish as scheduled.
Provide scheduled options and related model variants as indicated.
The manufacturer shall provide published performance data for the bar linear register, which shall be tested in accordance with ANSI/ASHRAE Standard 70-2023.
STANDARD FEATURES
· Fixed bars parallel to long dimension unless otherwise scheduled
· Reinforced heavy-duty core with additional supports every 2 in.
· Designed for floor or reinforced sidewall, sill, and ceiling applications
· Fully extruded architectural aluminum construction
· 1/2 in. standard dimensions; custom sizes to 1/16 in. increments
RELATED OPTIONS / MODEL VARIANTS
· Opposed blade damper with concealed operator
· DAPHN - No-flange heavy-duty grille
· DAPHC - Heavy-duty core only
· DAPH-TB - No mounting / No screw-hole option where scheduled
Note: Confirm listed size/opening size, outside size, or inside size as applicable; finish; mounting method; damper/filter/screen requirements; and current Dayus model availability before issuing project specifications.


	DABLS
	SHALLOW BAR LINEAR GRILLE

	TYPE: shallow bar linear grille
	CONSTRUCTION / BLADE: fixed bars parallel to the long dimension unless otherwise scheduled; blade option selected from -00, -01, -15, -30, -82, or -84 FLAGGED
	DAMPER / FILTER / SCREEN: none

	FRAME: fully extruded architectural aluminum, standard extruded aluminum frame, slim 1/2 in. deep profile
	FINISHES: White; Silver; Mill; Brown; Flat Black; Prime Coat; Special Order
	PERFORMANCE BASIS: ANSI/ASHRAE Standard 70-2023

	SUGGESTED SPECIFICATION:
Furnish and install Dayus Model DABLS Shallow Bar Linear Grille of the type, finish, scheduled listed size/opening size, outside size, or inside size as applicable, and mounting method shown on the plans and air distribution schedules.
The shallow bar linear grille shall be constructed with fully extruded architectural aluminum standard frame with slim 1/2 in. deep profile and fixed bars parallel to the long dimension unless otherwise scheduled; blade option selected from -00, -01, -15, -30, -82, or -84.
Units shall be furnished in Dayus [White; Silver; Mill; Brown; Flat Black; Prime Coat; Custom] finish as scheduled.
Provide scheduled options and related model variants as indicated.
The manufacturer shall provide published performance data for the bar linear grille, which shall be tested in accordance with ANSI/ASHRAE Standard 70-2023.

	STANDARD FEATURES
• Slim 1/2 in. deep design
• Fixed bars parallel to long dimension
• Selectable 2, 3, 4, or 6 in. height
• Fully extruded architectural aluminum construction
• Not designed for floor use
• 1/2 in. standard dimensions; custom sizes to 1/16 in. increments
	RELATED OPTIONS / MODEL VARIANTS



Specifier note: Confirm listed size/opening size, outside size, or inside size as applicable; finish; mounting method; damper/filter/screen requirements; and current Dayus model availability before issuing project specifications.
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