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DAPHN 
HEAVY DUTY BAR LINEAR GRILLE WITH NO FLANGE

TYPE: Heavy duty bar linear grille.
BLADE ARRANGEMENT: Fixed bars parallel to the long dimension unless otherwise scheduled; blade option selected from -00, -01, -15, -30, -82, or -84.
DAMPER / FILTER / SCREEN: None. 
FRAME: Fully extruded architectural aluminum, no-flange frame, reinforced heavy-duty core with additional supports.
FINISHES: W White; S Silver; M Mill; B- Brown; FB – Flat Black; P – Prime Coat; Special Order.
PERFORMANCE BASIS: ANSI/ASHRAE Standard 70-2023
SUGGESTED SPECIFICATION
Furnish and install Dayus Model DAPHN Heavy Duty Bar Linear Grille with No Flange of the type, finish, scheduled listed size/opening size, outside size, or inside size as applicable, and mounting method shown on the plans and air distribution schedules.
The heavy-duty bar linear grille shall be constructed with fully extruded architectural aluminum no-flange frame, reinforced heavy-duty core with additional supports and fixed bars parallel to the long dimension unless otherwise scheduled; blade option selected from -00, -01, -15, -30, -82, or -84.
Units shall be furnished in Dayus [White; Silver; Mill; Brown; Flat Black; Prime Coat; Custom] finish as scheduled.
Provide scheduled options and related model variants as indicated.
The manufacturer shall provide published performance data for the bar linear grille, which shall be tested in accordance with ANSI/ASHRAE Standard 70-2023.
STANDARD FEATURES
· No-flange frame for clean built-in appearance
· Fixed bar blades, direction as scheduled
· Heavy-duty reinforced core suitable for floor, sill, sidewall, or ceiling use
· Six blade profile options: -00, -01, -15, -30, -82, -84
· Fully extruded architectural aluminum construction
· 1/2 in. standard dimensions; custom sizes to 1/16 in. increments
RELATED OPTIONS / MODEL VARIANTS
· Mounting by Screw holes, Spring clips, Concealed brackets, Sidewall screws, or No mounting as scheduled
· See listed model variants as scheduled
· Heavy-duty core variants and no-flange/core-only options
Note: Confirm listed size/opening size, outside size, or inside size as applicable; finish; mounting method; damper/filter/screen requirements; and current Dayus model availability before issuing project specifications. 
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