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DARE5-FG
1" EGGCRATE FILTER GRILLE

TYPE: 1 in. eggcrate blade face filter grille.
BLADE ARRANGEMENT: Aluminum eggcrate core; face angle as scheduled.
DAMPER / FILTER / SCREEN: Integral filter frame for 1 in. filter; mounting selected as scheduled.
FRAME: Architectural aluminum extruded frame with roll-formed blades and eggcrate face.
FINISHES: W White; S Silver; M Mill.
PERFORMANCE BASIS: ANSI/ASHRAE Standard 70-2023
SUGGESTED SPECIFICATION
Furnish and install Dayus Model DARE5-FG 1" Eggcrate Filter Grille of the type, finish, scheduled listed size/opening size, outside size, or inside size as applicable, and mounting method shown on the plans and air distribution schedules.
The eggcrate face filter grille shall be constructed with architectural aluminum extruded filter frame with eggcrate face and aluminum eggcrate core; face angle as scheduled.
The unit shall include an integral filter frame for 1 in. filter; mounting selected as scheduled.
Units shall be furnished in Dayus [W White; S Silver; M Mill] finish as scheduled.
Provide scheduled options and related model variants as indicated.
The manufacturer shall provide published performance data for the eggcrate filter grille, which shall be tested in accordance with ANSI/ASHRAE Standard 70-2023.
STANDARD FEATURES
· Aluminum eggcrate core
· Accommodates a standard 1 in. filter
· Top and bottom mounting options: Spring Pins, Wire Hinge, Nylon Thumb Screw, Nylon Screen Tabs, or Security Screws as scheduled
· Recommended top mounting: Spring Pins or Wire Hinge only
· Available on 2 in. standard dimensions; custom sizes to 1/16 in. increments
RELATED OPTIONS / MODEL VARIANTS
· Spring Pin, Wire Hinge, Nylon Thumb Screw, Nylon Screen Tab, or Security Screw bottom mounting as scheduled; use Spring Pin or Wire Hinge for top mounting
· T-bar ceiling frame variant available where scheduled
· 2 in or 4 in. filter depth variants
Note: Confirm listed size/opening size, outside size, or inside size as applicable; finish; mounting method; damper/filter/screen requirements; and current Dayus model availability before issuing project specifications.
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