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Return Grilles & Registers



DARH-SD
RETURN AIR REGISTER WITH 0° DEFLECTION

TYPE: Return register.  
BLADE ARRANGEMENT: Semi-airfoil horizontal blades, fixed 0°, on 2/3 in. spacing.
DAMPER / FILTER / SCREEN: Opposed blade damper adjustable from face using a slender tool.
FRAME: Architectural aluminum extruded frame with roll-formed blades.
FINISHES: W White; S Silver; M Mill.
PERFORMANCE BASIS: ANSI/ASHRAE Standard 70-2023
SUGGESTED SPECIFICATION
Furnish and install Dayus Model DARH-SD Return Air Register with 0° Deflection of the type, finish, scheduled listed size/opening size, outside size, or inside size as applicable, and mounting method shown on the plans and air distribution schedules.
The Return register shall be constructed with architectural aluminum extruded frame with roll-formed blades and semi-airfoil horizontal blades, fixed 0°, on 2/3 in. spacing.
The unit shall include an opposed blade damper with concealed operator design.
Units shall be furnished in Dayus [W White; S Silver; M Mill] finish as scheduled.
Provide scheduled options and related model variants as indicated.
The manufacturer shall provide published performance data for the return register, which shall be tested in accordance with ANSI/ASHRAE Standard 70-2023.
STANDARD FEATURES
· Fixed 0° deflection on 2/3 in. blade spacing
· Extruded aluminum frame with roll-formed aluminum blades
· Pressure-fitted blades for rattle-free performance
· 2 in. standard dimensions; custom sizes to 1/16 in. increments
RELATED OPTIONS / MODEL VARIANTS
· No mounting / No screw-hole option
· Insect screen where scheduled
· All aluminum construction
· 1 in. blade spacing, 0° deflection, adjustable blade, or opposed damper variants where scheduled
Note: Confirm listed size/opening size, outside size, or inside size as applicable; finish; mounting method; damper/filter/screen requirements; and current Dayus model availability before issuing project specifications.



image1.png




image2.png




