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Return Grilles & Registers



DARHED-30
30° EXTRUDED RETURN AIR REGISTER

TYPE: Return register.  
BLADE ARRANGEMENT: Fully extruded fixed blades at 30° on 3/4 in. spacing.
DAMPER / FILTER / SCREEN: Opposed blade damper adjustable from face using a slender tool.
FRAME: Fully extruded architectural aluminum frame.
FINISHES: W White; S Silver; M Mill; B Brown; FB Flat Black; Prime Coat; Special Order
PERFORMANCE BASIS: ANSI/ASHRAE Standard 70-2023
SUGGESTED SPECIFICATION
Furnish and install Dayus Model DARHED-30 30° Extruded Return Air Register of the type, finish, scheduled listed size/opening size, outside size, or inside size as applicable, and mounting method shown on the plans and air distribution schedules.
The Return register shall be constructed with fully extruded architectural aluminum frame and fully extruded fixed blades at 30° on 3/4 in. spacing.
The unit shall include an opposed blade damper with concealed operator design.
Units shall be furnished in Dayus [W White; S Silver; M Mill; B Brown; FB Flat Black; Prime Coat; Special Order] finish as scheduled.
Provide scheduled options and related model variants as indicated.
The manufacturer shall provide published performance data for the return register, which shall be tested in accordance with ANSI/ASHRAE Standard 70-2023.
STANDARD FEATURES
· Fixed 30° deflection on 3/4 in. blade spacing
· Fully extruded architectural aluminum construction
· Hidden supports for clean appearance
· 2 in. standard dimensions; custom sizes to 1/16 in. increments
RELATED OPTIONS / MODEL VARIANTS
· No mounting / No screw-hole option
· Bird screen or insect screen where scheduled
· All aluminum construction
· Alternate 30° / 45° deflection models
· Opposed blade damper register variant where scheduled
Note: Confirm listed size/opening size, outside size, or inside size as applicable; finish; mounting method; damper/filter/screen requirements; and current Dayus model availability before issuing project specifications.
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