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DASLR
SLOT LINEAR RETURN

TYPE: Slot linear return.
BLADE ARRANGEMENT: Linear return slot face designed to match active DASL diffuser sections.
DAMPER / FILTER / SCREEN: None.
FRAME: Fully extruded high-quality aluminum frame.
FINISHES: W White; FB – Flat Black.
PERFORMANCE BASIS: ANSI/ASHRAE Standard 70-2023
SUGGESTED SPECIFICATION
Furnish and install Dayus Model DASLR Slot Linear Return of the type, finish, scheduled listed size/opening size, outside size, or inside size as applicable, and mounting method shown on the plans and air distribution schedules.
The slot linear return shall be constructed with fully extruded high-quality aluminum frame and linear return slot face designed to match active DASL diffuser sections.
Units shall be furnished in Dayus [White; Flat Black] finish as scheduled.
Provide scheduled options and related model variants as indicated.
The manufacturer shall provide published performance data for the slot linear return section, which shall be tested in accordance with ANSI/ASHRAE Standard 70-2023.
STANDARD FEATURES
· Fully extruded aluminum construction
· Inactive return sections match active slot diffuser sections
· Available in any length
· Lengths over 84 in. joined with alignment pins for continuous appearance
· 1/2 in. standard dimensions; custom sizes to 1/16 in. increments
RELATED OPTIONS / MODEL VARIANTS
· DASL - Matching standard-frame active diffuser
· DASLRJ - Mud-in frame return/inactive section
· DASLJ - Matching mud-in active diffuser
Note: Confirm listed size/opening size, outside size, or inside size as applicable; finish; mounting method; damper/filter/screen requirements; and current Dayus model availability before issuing project specifications. 
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