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DASLRJ
SLOT LINEAR RETURN WITH MUD-IN FLANGE

TYPE: Slot linear return with mud-in flange. 
BLADE ARRANGEMENT: Linear return slot face designed to match active DASL diffuser sections.
DAMPER / FILTER / SCREEN: None.
FRAME: Fully extruded high-quality aluminum with recessed mud-in flange.
FINISHES: W White; FB – Flat Black.
PERFORMANCE BASIS: ANSI/ASHRAE Standard 70-2023
SUGGESTED SPECIFICATION
Furnish and install Dayus Model DASLRJ Slot Linear Return with mud-in flange of the type, finish, scheduled listed size/opening size, outside size, or inside size as applicable, and mounting method shown on the plans and air distribution schedules.
The slot linear return with mud-in flange shall be constructed with fully extruded high-quality aluminum with recessed mud-in flange and linear return slot face designed to match active DASL diffuser sections.
Units shall be furnished in Dayus [White; Flat Black] finish as scheduled.
Provide scheduled options and related model variants as indicated.
The manufacturer shall provide published performance data for the slot linear return section, which shall be tested in accordance with ANSI/ASHRAE Standard 70-2023.
STANDARD FEATURES
· Mud-in recessed flange for tape-and-plaster concealed appearance
· Fully extruded aluminum construction
· Inactive return sections match active slot diffuser sections
· Available in any length
· Lengths over 84 in. joined with alignment pins for continuous appearance
· 1/2 in. standard dimensions; custom sizes to 1/16 in. increments
RELATED OPTIONS / MODEL VARIANTS
· DASLR - Standard frame return/inactive section
· DASLJ - Matching mud-in supply diffuser
· DASL - Standard frame supply diffuser
Note: Confirm listed size/opening size, outside size, or inside size as applicable; finish; mounting method; damper/filter/screen requirements; and current Dayus model availability before issuing project specifications. 
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