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Supply Grilles & Registers



DAV-WF
SINGLE DEFLECTION SUPPLY GRILLE WITH WIDE FLANGE - VERTICAL BLADE

MODEL DESCRIPTION: Wide flange for additional mounting surface coverage; vertical blade single-deflection supply grille.
TYPE: Supply grille.  
BLADE ARRANGEMENT: One set of individually adjustable, semi-airfoil vertical blades spaced on 2/3 in. centers
DAMPER: None.
FRAME: Wide-flange architectural aluminum frame.
FINISHES: W - White; S - Silver; M - Mill
PERFORMANCE BASIS: ANSI/ASHRAE Standard 70-2023
SUGGESTED SPECIFICATION
Furnish and install Dayus Model DAV-WF Single Deflection Supply Grilles of the type, finish, listed size/opening size, and mounting method shown on the plans and air distribution schedules. Units shall include a wide flange for additional mounting surface coverage. The grilles shall have one set of individually adjustable, semi-airfoil vertical blades spaced on 2/3 in. centers. The frame shall be architectural aluminum with roll-formed aluminum blades, pressure-fitted for rattle-free performance, and supplied with a sealing gasket to help prevent streaking on walls or ceilings. Units shall be furnished in Dayus W White, S Silver, or M Mill finish as scheduled.
(Optional) No screw-hole fastening and all-aluminum construction shall be provided where scheduled. For applications requiring volume control, provide Dayus Model DAVD-WF as scheduled.
The manufacturer shall provide published performance data for the grille or register, which shall be tested in accordance with ANSI/ASHRAE Standard 70-2023.
STANDARD FEATURES
· Wide flange for additional mounting surface coverage
· Architectural aluminum construction with extruded frame and roll-formed blades
· Pressure-fitted blades for rattle-free performance
· Sealing gasket to help prevent streaking on walls or ceilings
· Available on 2 in. standard dimensions; custom sizes manufactured up to 1/16 in. increments.
RELATED OPTIONS / MODEL VARIANTS
· DAVD-WF - Opposed blade damper
· DAV-WF-TB - No screw holes
· DAV-WF-AA - All aluminum construction
· DAH-WF - Horizontal blade version
Note: Use bracketed finish, size, mounting, and option selections from the project plans and air distribution schedule.
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