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Supply Grilles & Registers



DAVHD
DOUBLE DEFLECTION SUPPLY REGISTER - VERTICAL FRONT - OBD

MODEL DESCRIPTION: Double deflection aluminum register with vertical front blades, horizontal rear blades, and opposed blade damper.
TYPE: Supply register.
BLADE ARRANGEMENT: Two sets of individually adjustable, semi-airfoil blades spaced on 2/3 in. centers; vertical front blades and horizontal rear blades. 
DAMPER: Opposed blade damper with concealed operator design. 
FRAME: Standard architectural aluminum frame.
FINISHES: W - White; S - Silver; M – Mill
PERFORMANCE BASIS: ANSI/ASHRAE Standard 70-2023
SUGGESTED SPECIFICATION
Furnish and install Dayus Model DAVHD Double Deflection Supply Registers of the type, finish, listed size/opening size, and mounting method shown on the plans and air distribution schedules. The registers shall have two sets of individually adjustable, semi-airfoil blades spaced on 2/3 in. centers, with vertical front blades and horizontal rear blades for two-plane air-direction control. The frame shall be architectural aluminum with roll-formed aluminum blades, pressure-fitted for rattle-free performance, and supplied with a sealing gasket to help prevent streaking on walls or ceilings. The register shall include an opposed blade damper with concealed operator design for volume control. Units shall be furnished in Dayus W White, S Silver, or M Mill finish as scheduled.
(Optional) No screw-hole fastening and all-aluminum construction shall be provided where scheduled. Where a damper is not required, provide Dayus Model DAVH.
The manufacturer shall provide published performance data for the grille or register, which shall be tested in accordance with ANSI/ASHRAE Standard 70-2023.
STANDARD FEATURES
· Two sets of individually adjustable, semi-airfoil blades with vertical front blades and horizontal rear blades on 2/3 in. spacing
· Architectural aluminum construction with extruded frame and roll-formed blades
· Pressure-fitted blades for rattle-free performance
· Sealing gasket to help prevent streaking on walls or ceilings
· Available on 2 in. standard dimensions; custom sizes manufactured up to 1/16 in. increments.
RELATED OPTIONS / MODEL VARIANTS
· DAVHD-TB - No screw holes
· DAVHD-AA - All aluminum construction
· DAVH - No damper
· DAHVD - Horizontal front version
Note: Use bracketed finish, size, mounting, and option selections from the project plans and air distribution schedule.



image1.png




image2.png




